Data/hora: 19/05/2024 17:05:15

Biblioteca(s): 	Embrapa Florestas.	
Data corrente: 	01/10/2015	
Data da última atualização: 	29/01/2018	
Autoria: 	LOURENÇON, T. V.; HANSEL, F. A.; SILVA, T. A. da; RAMOS, L. P.; BOLZON DE MUNIZ, G. I.; MAGALHAES, W. L. E.	
Afiliação: 	TAINISE V. LOURENÇON, Doutoranda UFPR; FABRICIO AUGUSTO HANSEL, CNPF; THIAGO A. DA SILVA, UFPR; LUIZ P. RAMOS, UFPR; GRACIELA I. BOLZON DE MUNIZ, UFPR; WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF.	
Título: 	Hardwood and softwood kraft lignins fractionation by simple sequential acid precipitation.	
Ano de publicação: 	2015	
Fonte/Imprenta: 	Separation and Purification Technology, v. 154, p. 82-88, Nov. 2015.	
DOI: 	http://dx.doi.org/10.1016/j.seppur.2015.09.015	
Idioma: 	Inglês	
Conteúdo: 	This study aimed at the fractionation of lignin by a simple acid precipitation from hardwood and softwood Kraft black liquors to propose new value-added applications. The precipitation was made sequentially by acidification at five different pHs (9, 7, 5, 3 and 1). The different lignin fractions were analyzed in terms of yield, ash content, elemental analysis, thermal analysis, FTIR, 1H NMR and GPC. Hardwood lignins showed distinct relative molecular mass distributions, while softwood lignins showed similar relative molecular mass distributions in the three fractions obtained at higher pHs (pH 9, 7 and 5). This simple acid precipitation was shown to be an effective method to obtain relatively high yields of lignin. Molecular characterization by FTIR (carbonyl band) indicated that hardwood lignin was most oxidized mainly in the low pH fractions (5, 3 and 1), while the softwood lignin only presented discrete oxidized products in the lowest pHs (3 and 1). Interestingly, precipitation at pH 3 produced ash-free hardwood and softwood lignin fractions, which is a valuable product for the development of better end uses.	
Thesagro: 	Eucalipto; Lignina; Madeira.	
Thesaurus Nal: 	Pinus.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (54309-1) - UPC - AP - DD -  -  -  - DIS