Data/hora: 09/06/2024 11:59:53

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	19/01/2006	
Data da última atualização: 	19/01/2006	
Autoria: 	CONSOLIN FILHO, N.; MEDEIROS, E. S.; TANIMOTO, S. T.; MATTOSO, L. H.	
Título: 	Sensors of conducting polymers for detection of pesticides in contaminated water.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	In: INTERNATIONAL SYMPOSIUM ON ELECTRETS, 12.; 2005, Salvador. Proceedings... Salvador: IEEE, 2005. p. 424-427.	
Idioma: 	Inglês	
Conteúdo: 	A sensor arrqy composed by different sensing materials, vi., poly(o-ethoxyaniline), polyaniline, lignin and humic substance, was used to study the contamination levels in water by pesticides. This array was characterized by electrical measurements (electrochemical impedance spectroscopy), atomic force microscopy and ultraviolet-visible spectrophometry.	
Palavras-Chave: 	Humic substance; Poly(o-ethoxyaniline).	
Thesaurus Nal: 	pesticides.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9181-1) - UPC - SP - -- - PROCI-05.00025 -  - 2005.00025 - DIS