Data/hora: 26/05/2024 10:31:48

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 22/12/1999
Data da última atualização: | 22/12/1999
Autoria: | ASSIS, O. B. G.; CRNKOVIC, F. C.; MACHADO, R.; AVACA, L. A.; FERRANTE, M.; MACHADO, S. A. S.
Afiliação: | EMBRAPA-CNPDIA; USP-IQSC-GMEME; UFSCar-CCDM; UFSCar-DEMa.
Título: | Powder metallurgy processing of Ni-Co base electrodes for application in water electrolysis.
Ano de publicação: | 1997
Fonte/Imprenta: | In: INTERNATIONAL LATIN-AMERICAN CONFERENCE ON POWDER TECHNOLOGY=CONFERENCIA INTERNACIONAL LATINO-AMERICANA EM TECNOLOGIA DO PO, 1., Nov. 1997, Aguas de Lindoia, SP. Information/Informativo... Aguas de Lindoia: Associacao Brasileira de Ceramica, 1997.
Páginas: | não paginado.
Idioma: | Inglês
Conteúdo: | Electrodes of Co, Ni and Ni50Co50 were produced by pwder metallurgy techniques aaiming at their application as cathodes for water electrolyssis system. Sintering was carried out in vacuum/argon atmosphere at low temperature in order to enhance surface electroactivity by an increase if the geometric area. The Ni-Co alloyng was obtained by mechanical synthesis, making use of the appropriated route. The final electrodes presented porosity of around 12% where the electrochemical tests presented increasing in the critical peak when compared with eletroplated flat samples.
Palavras-Chave: | Mechanical alloying; Sintering; Water electrolysis.
Thesaurus Nal: | electrochemistry.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (5643-1) - UPC - SP - -- - PROCI-97.00008 -  - 1997.00008 - DIS