Data/hora: 27/05/2024 05:22:36

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 20/08/2003
Data da última atualização: | 08/05/2008
Autoria: | MARTINS, M. A.; MATTOSO, L. H. C.
Afiliação: | Embrapa Instrumentação Agropecuária, São Carlos, SP.
Título: | Tire rubber/sisal fiber composites: effect of the chemical treatment and fiber length on viscoeleastic properties.
Ano de publicação: | 2002
Fonte/Imprenta: | In: SIMPOSIO LATINOAMERICANO DE POLÍMEROS, 8.; CONGRESO IBEROAMERICANO DE POLÍMEROS, 6.; SIMPÓSIO IBEROAMERICANO DE QUITINA, 2.; CONGRESO NACIONAL DE POLÍMEROS, 15., 2002, Acapulco. SLAP' 2002: libro de resúmenes. Acapulco: Sociedad Polimerica de Mexico A. C., 2002. p. 280-281. MC-II-1.
Idioma: | Inglês
Conteúdo: | In this work, the effects of fiber treatments (mercerization and acetylation), fiber length, and temperature on the mechanical and dynamic  mechanical properties of tire rubber/sisal fiber composites were studied.
Palavras-Chave: | Fiber treatment; New materials; Novos materiais; Rubber fiber composites; Sisal fiber composites.
Thesagro: | Borracha; Sisal.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (7950-1) - UPC - SP - -- - PROCI-02.00099 -  - 2002.00099 - DIS