Data/hora: 11/06/2024 09:13:31

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 14/02/2006
Data da última atualização: | 14/02/2006
Autoria: | MORENO, R. M. B.; MEDEIROS, E. S. de; FERREIRA, F. C.; ALVES, N.; GONÇALVES, P. S.; MATTOSO, L. H. C.
Título: | Thermogravimetric studies of decomposition kinetics of six different IAC Hevea rubber clones using Flynn-Wall-Ozawa approach.
Ano de publicação: | 2006
Fonte/Imprenta: | Plastics, Rubber and Composites, v.35, n.1, 2006.
Idioma: | Inglês
Conteúdo: | The thermal degradation behaviour of rubber from six new Hevea brasiliensis clones (IAC 40, 56, 300, 301, 302 and 303) from São Paulo State, Brazil was studied by thermogravimetry using the Flynn-Wall-Ozawa approach to assess the kinetic parameters (reaction order, activation energy and pre-exponential factor) of the decomposition process. This study indicated that the thermal behaviour is a complex multiple step process, which dependes on the type of rubber Hevea clones studied. The rubber from these clones can be classified, following the order of decreasing thermal stability, as IAC 303 >302 >56 >40 >300 >301.
Palavras-Chave: | Degradation kinetics; Flynn-Wall-Ozawa approach; Rubber Hevea clones.
Thesaurus Nal: | thermogravimetry.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9409-1) - UPC - SP - -- - PROCI-06.00001 -  - 2006.00001 - DIS