Data/hora: 13/06/2024 09:05:41

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	24/03/2006	
Data da última atualização: 	24/03/2006	
Autoria: 	POSADAS, A. N.; CRESTANA, S.	
Título: 	3-D wetting front instabilities in layered soil studies using MRI and an invasion percolation model.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	In: AMERICAN SOCIETY OF AGRONOMY ANNUAL MEETING, 91., 1999, Salt Lake City. 1999 Annual meeting abstracts... New York: ASA: CSSA: SSSA, 1999. p.305-309.	
Idioma: 	Inglês	
Conteúdo: 	This work presents a three-dimensional characterization and simulation of preferential flow in a two-layer soilusing Magnetic Resonance Imaging-MRI, fractal theory, and an invasion percolation model. The infiltration process ofwater through a stratified sandy soil column was studied under hydrodynamics steady state condition with imagesobtained using a 500 Gauss MRI system.	
Palavras-Chave: 	Imagem; MRI; Três dimensões.	
Thesaurus Nal: 	magnetic resonance imaging.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9649-1) - UPC - SP - -- - PROCI-99.00131 -  - 1999.00131 - DIS