Data/hora: 03/06/2024 10:07:10

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 12/12/2005
Data da última atualização: | 06/05/2008
Autoria: | TORRE-NETO, A.; SCHUELLER, J. K.; HAMAN, J. K.
Título: | Automated system for variable rate microsprinkler irrigation in citrus: a demostration unit.
Ano de publicação: | 2001
Fonte/Imprenta: | In: EUROPEAN CONFERENCE ON PRECISION AGRICULTURE-ECPA, 3.; EUROPEAN CONFERENCE OF THE EUROPEAN FEDERATION FOR INFORMATION TECHNOLOGY IN AGRICULTURE, FOOD AND ENVIRONMENT-EFITA, 3., 2001, Montpellier. Third European Conference... Montpellier: Ecole National Supérieure Agronomique, 2001. p. 725-730. 1 CD-ROM.
Idioma: | Inglês
Conteúdo: | An automated system was developed using soil probes with temperature and matric potencial sensors to measure spatially-variable soil conditions and to spatially-variably control microsprinkler irrigation by local or remote operation using an Rs-485 network. The system was successfully constructed, installed, and demonstrated in a small citrus grove.
Palavras-Chave: | RS-485; Sensors.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9076-1) - UPC - SP - -- - PROCI-01.00149 -  - 2001.00149 - DIS