Data/hora: 01/06/2024 17:52:06

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	23/03/2005	
Data da última atualização: 	23/03/2005	
Autoria: 	SIMÕES, F. R.	
Título: 	New electrode material for the electrochemical determination of 2,4 Diclorophenoxyacetic acid herbicide (2,4D).	
Ano de publicação: 	2003	
Fonte/Imprenta: 	In: ENCONTRO DA SOCIEDADE BRASILEIRA DE PESQUISA EM MATERIAIS, SBPMAT, 2., out. 2003., Rio de Janeiro, RJ. Programa e Livro de resumos... Rio de Janeiro: SBPMat, 2003. Ref. A-P49.	
Idioma: 	Inglês	
Conteúdo: 	Conducting polymers have been used in many technological and scientific research applications. Due to the necessity of active materiais and great demand for different applications, the conducting polymer allows an increasing of versatility for the construction of sensors. In agriculture, in particular, the uncontrolled use of pesticide has been causing a great environmental impact, as for example the groundwater and surface water contamination. The most popular methods of pesticide analysis are the chromatographics mainly the HPLC and gas chromatography. These methods are sensible and selective, but they are laborious and expensive. Electroanalytical techniques have aIso been used as methods for pesticides determination in natural waters, soils, vegetables, fruits and other matrices. The main advantage of this method is the possibility of determining its concentration without previous treatments or separations. This work presents a new modified electrode for the determination of the herbicide 2,4 diclorophenoxyacetic acid (2,4D). This compound is known as not electroactive in electrodes as mercury, platinum and carbon (glassy, fiber or paste), but a new composite material consisting of carbon paste electrode and the conducting polymer polyaniline (PANI) was prepared, showing electroactivy and therefore, the possibility of the pesticide determination using electrochemical techniques. The analyses of the herbicide was carried out through cyclic voltammetry (C. V) in different pHs. The results showed good sensitivity and selectivity. 	
Palavras-Chave: 	Pesticidas; Polímeros condutores.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8746-1) - UPC - SP - -- - PROCI-03.00091 -  - 2003.00091 - DIS