Data/hora: 31/05/2024 02:20:29

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 01/02/2006
Data da última atualização: | 01/02/2006
Autoria: | STOLF, R.; REICHARDT, K.; VAZ, C. M. P.
Título: | Response to "Commens on 'Simultaneous measurement of soil penetration resistance and water content with a combines penetrometer - TDR moisture probe' and ' A dynamic cone penetrometer for measuring soil penetratiom resistance'.
Ano de publicação: | 2005
Fonte/Imprenta: | Soil Science Society of America Journal, Madison, v. 69, p. 925-926, May 6, 2005. Disponível em: <http://soil.scijournals.org/content/vol69/issue3/#COMMENTS_AND_LETTERS_TO_THE_EDITOR>. Acesso em: 11 jan. 2006. Acesso restrito.
Idioma: | Inglês
Conteúdo: | My coauthor and I would like to thank Dr. Minasny and Dr. McBratney for their perceptive comments. We concur that by accounting for momentum, their Eq. [8] may more accurately reflect the energy transmitted form the sliding hammer to the penetrometer described in Herrick and Jones (2002).
Palavras-Chave: | Penetrometer; Resposta para comentário.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9379-1) - UPC - SP - -- - PROCI-05.00115 -  - 2005.00115 - DIS