Data/hora: 25/05/2024 14:58:23

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	01/02/2006	
Data da última atualização: 	01/02/2006	
Autoria: 	STOLF, R.; REICHARDT, K.; VAZ, C. M. P.	
Título: 	Response to "Commens on 'Simultaneous measurement of soil penetration resistance and water content with a combines penetrometer - TDR moisture probe' and ' A dynamic cone penetrometer for measuring soil penetratiom resistance'.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	Soil Science Society of America Journal, Madison, v. 69, p. 925-926, May 6, 2005. Disponível em: <http://soil.scijournals.org/content/vol69/issue3/#COMMENTS_AND_LETTERS_TO_THE_EDITOR>. Acesso em: 11 jan. 2006. Acesso restrito.	
Idioma: 	Inglês	
Conteúdo: 	My coauthor and I would like to thank Dr. Minasny and Dr. McBratney for their perceptive comments. We concur that by accounting for momentum, their Eq. [8] may more accurately reflect the energy transmitted form the sliding hammer to the penetrometer described in Herrick and Jones (2002).	
Palavras-Chave: 	Penetrometer; Resposta para comentário.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9379-1) - UPC - SP - -- - PROCI-05.00115 -  - 2005.00115 - DIS