Data/hora: 23/05/2024 16:12:21

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	03/02/2006	
Data da última atualização: 	03/02/2006	
Autoria: 	VENANCIO, T.; ENGELSBERG, M.; AZEREDO, R. B. V. de, COLNAGO, L. A.	
Título: 	CWFP as a tool for fast and simultaneous measurement of t1 and t2 relaxation times.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	In: WOKSHOP DA PÓS-GRADUAÇAO, 9.; 2005, São Carlos. A contribuição do IQSC para a inovação e o desenvolvimento científico e tecnológico. Resumos... São Carlos: IQSC, 2005. p. 39.	
Idioma: 	Inglês	
Conteúdo: 	A recent version of this method proposes that the time-consuming determination of the first step can be bypassed, permitting the simultaneous and fast measurement of T1 and T2 in sigle continuous wave free precession (CWFP) experiment, taking account the role of an inhomogeneous magnetic field and its effect on the measured relaxation times is examined pointing out possible sources of error.	
Palavras-Chave: 	CWFP; NMR relaxation times; SSFP.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9387-1) - UPC - SP - -- - PROCI-05.00124 -  - 2005.00124 - DIS