Data/hora: 23/05/2024 04:00:57

Biblioteca(s): 	Embrapa Florestas.	
Data corrente: 	09/12/2016	
Data da última atualização: 	11/07/2017	
Autoria: 	LOUREÇON, T. V.; MATTOS, B. D.; CADEMARTORI, P. H. G.; MAGALHAES, W. L. E.	
Afiliação: 	Tainise V. Lourençon, Doutoranda da UFPR, Centro de Ciências Florestais e da Madeira; Bruno D. Mattos, Doutorando da UFPR, Programa Integrado de Engenharia e Ciência dos Materiais; Pedro H. G. Cademartori, Doutorando da UFPR, Centro de Ciências Florestais e da Madeira; WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF.	
Título: 	Bio-oil from a fast pyrolysis pilot plant as antifungal and hydrophobicagent for wood preservation.	
Ano de publicação: 	2016	
Fonte/Imprenta: 	Journal of Analytical and Applied Pyrolysis, v. 122, p. 1-6, Nov. 2016.	
DOI: 	http://dx.doi.org/10.1016/j.jaap.2016.11.004	
Idioma: 	Inglês	
Conteúdo: 	Residual wood fines were used as raw material to produce fast pyrolysis bio-oil in a pilot plant for furtherutilization as antifungal and hydrophobic agent for wood protection. Phenolic compounds derived fromlignin mostly composed the obtained bio-oil. Pinewood was impregnated with natural and diluted bio-oilaiming three different final loads. Scanning electron microscopy images revealed that the internal surfaceof the tracheids was coated by the bio-oil. Fourier-transformed infrared analysis showed no chemicalreactions between wood and bio-oil, while thermogravimetric studies stated changes in the thermalstability of the impregnated pinewood. The bio-oil impregnation proved to be effective to decrease thewater absorption and wettability of the pinewood. In addition, the bio-oil impregnated pinewood withlow load (7.95%) had decay resistance improved by 2.6 and 4.5 times against T. versicolor and G. trabeumfungi, respectively, meanwhile the highest bio-oil loading (81.3%) inside pinewood caused the mortalityof the whole fungal colony in the first days of test.	
Palavras-Chave: 	Bio oil; Bio óleo; Repelência à água; Water repellence.	
Thesagro: 	Madeira; Preservação da Madeira.	
Thesaurus Nal: 	decay resistance; phenolic compounds; Wood preservation.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (55425-1) - UPC - AP - DD -  -  -  - DIS