Data/hora: 23/06/2024 10:26:35

Biblioteca(s): 	Embrapa Agricultura Digital.	
Data corrente: 	18/01/2010	
Data da última atualização: 	15/03/2013	
Autoria: 	SANTOS, G. A. dos; DIAS JUNIOR, M. de S.; GUIMARÃES, P. T. G.; ARAÚJO JUNIOR, C. F.; PAIS, P. S'A. M.	
Afiliação: 	GISLENE APARECIDA DOS SANTOS, UFLA; MOACIR DE SOUZA DIAS JUNIOR, UFLA; PAULO TÁCITO GONTIJO GUIMARÃES, EPAMIG; CEZAR FRANCISCO ARAÚJO JUNIOR, UFLA; PAULA SANT' ANNA MOREIRA PAIS, SAPC, UFLA.	
Título: 	Weed management and its influence on the load bearing capacity of red-yellow latosol under the crown projection in coffee culture.	
Ano de publicação: 	2009	
Fonte/Imprenta: 	Coffee science, Lavras, v. 4, n. 2, p. 165-177, jul./dez. 2009.	
Idioma: 	Inglês	
Notas: 	Part of the Doctoral Thesis of the first author, presented to DCS/UFLA. Project financed by EMBRAPA-CAFÉ and FAPEMIG.	
Conteúdo: 	Weed management is identified as a major cause of soil compaction in coffee plantations, because of its necessary frequent undertaking. The objectives of this study were: a) to develop bearing capacity models, for a Red-Yellow Latosol cultivated with coffee (Coffea arabica, L.), as a function of the associated weed management methods, preconsolidation pressure and moisture; b) to identify, through the use of these models, the weed management more resistant and more susceptible to soil compaction, under the coffee crown projection. This study was carried out in an experiment installed in the Experimental Farm of EPAMIG in Patrocínio MG, using the Rubi cultivar 1192. The weed control methods were: Hand hoe, Post-emergence herbicide, Pre-emergence herbicide and Brush Trimmer (Roçacarpa commercial name), associated with the rotary tiller, disk harrow, were mower and no weed control between plant rows. For each weed management, 15 samples were collected at depths of 0-3, 10-13 and 25-28 cm, to generate the capacity bearing model, totaling 720 undisturbed soil samples. To obtain the capacity bearing models, the undisturbed soil samples with different moisture content were submitted to the uniaxial compression tests according to Bowles (1986) modified by Dias Junior (1994). The pre-emergence herbicide associated to no weed control condition and were mower and the hand hoe associated to no weed control presented higher resistance to soil compaction. The Brush Trimmer (Roçacarpa) methods, associated to were mower; the Pre-emergence herbicide, associated to rotary tillers; and Pre-emergence herbicide and Brush Trimmer, associated to disk harrow between rows, presented higher susceptibility to soil compaction.	
Palavras-Chave: 	Coffee; Lavoura cafeeira; Modelos de capacidade de suporte de carga; Plantas daninhas; Suscetibilidade à compactação; Weed.	
Thesagro: 	Café; Coffea Arábica.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Agricultura Digital (CNPTIA)	
Exemplares: 	CNPTIA - (14480-1) - ADD - AP - PP -  -  -  - DIS