Data/hora: 16/06/2024 01:15:26

Biblioteca(s): | Embrapa Agricultura Digital.
Data corrente: | 18/03/1998
Data da última atualização: | 03/08/2007
Autoria: | ANDRADE, M. C. de; BERTRAND, G.; EVERAT, J. C.; ARAUJO, A. de A.
Título: | Segmentation of ceramical micrographies by flooding simulation: a catchment basins merging algorithm.
Ano de publicação: | 1996
Fonte/Imprenta: | In: SIMPÓSIO BRASILEIRO DE COMPUTAÇÃO GRÁFICA E PROCESSAMENTO DE IMAGENS, 9., 1996, Caxambu. Anais... Caxambu: SBC, 1996.
Páginas: | p.355-356.
Idioma: | Inglês
Notas: | Evento conhecido como: SIBGRAPI. Editado por L. Velho, A. de Albuquerque e R. A. Lotufo.
Conteúdo: | This work addresses a catchment basins merging algorithm developed to automatize the segmentation of ceramical images. The proposed algorithm, which is a modification of the watershed algorithm, employs two parameters to control the cachment basins merging: a depth criterium and an area criterium. This solution suppresses the characteristic over-segmentation of the flooding simulation algorithm enabling the direct image segmentation. There is no need of a previous pre-processing step. It is shown that this solution produces excellent segmentation results.
Palavras-Chave: | Computacao grafica; Graphic computation; Image processing; Processamento de imagens.
Categoria do assunto: | --
Registro original: | Embrapa Agricultura Digital (CNPTIA)
Exemplares: | CNPTIA - (6747-1) - ADD - PL - -- - 006.6 - SIM - 1996.00014 - DIS