Data/hora: 23/09/2024 23:48:24

Biblioteca(s): 	Embrapa Gado de Leite.	
Data corrente: 	23/03/2009	
Data da última atualização: 	24/03/2023	
Autoria: 	OTENIO, M. H.; PANCHONI, L. C.; CRUZ, G. C. A.; RAVANHANI, C.; BIDÓIA, E. D.	
Afiliação: 	Marcelo Henrique Otênio, Embrapa Gado de Leite; Luciana Cadioli Panchoni, SAAE-PR; Gabriela Correia Araújo da Cruz, SAAE-PR; Clézio Ravanhani, SAAE-PR; Ederio Dino Bidóia, Unesp.	
Título: 	Avaliação em escala laboratorial da utilização do processo eletrolítico no tratamento de águas.	
Ano de publicação: 	2008	
Fonte/Imprenta: 	Química Nova, v. 31, n. 3, p. 508-813, 2008.	
Idioma: 	Português	
Conteúdo: 	Water treatment uses chlorine for disinfection causing formation of trihalomethanes. In this work, an electrolytic water pre-treatment was studied and applied to the water from a fountainhead. The action against microorganisms was evaluated using cast-iron and aluminum electrodes. Assays were made in laboratory using the electrolytic treatment. After 5 min of electrolysis the heterotrophic bacteria count was below 500 cfu/mL and complete elimination of total and fecal coliforms was observed. Using electrolytic treatment as a pretreatment of conventional tap water treatment is proposed.	
Palavras-Chave: 	Tratamento eletrolítico.	
Thesagro: 	Desinfecção; Qualidade da Água.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/596412/1/Avaliacao-em-escala-laboratorial.pdf	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (16326-1) - UPC - AP - DD -  -  -  - DIS