Data/hora: 22/06/2024 03:20:15

Biblioteca(s): | Embrapa Agrossilvipastoril.
Data corrente: | 07/02/2018
Data da última atualização: | 07/02/2018
Autoria: | DURKS, J. M.; BOTELHO, F. M.; BOTELHO, S. de C. C.; ALMEIDA, L. C. B. de.
Afiliação: | JULIANA MEGIER DURKS, UFMT-SINOP; FERNANDO MENDES BOTELHO, UFMT-SINOP; SILVIA DE CARVALHO CAMPOS BOTELHO, CPAMT; LAYANNE CRISTINA BUENO DE ALMEIDA, UFMT-SINOP.
Título: | Perdas em grãos de soja armazenados.
Ano de publicação: | 2017
Fonte/Imprenta: | In: CONGRESSO BRASILEIRO DE ENGENHARIA AGRÍCOLA, 46., 2017, Maceió. Anais.. Maceió: SBEA, 2017.
Idioma: | Português
Conteúdo: | PT-BR: Objetivou-se com o presente trabalho avaliar as perdas qualitativas e quantitativas durante o período de armazenamento de grãos de soja. Foram utilizados grãos de soja produzidos e armazenados no município de Sorriso ? MT. Avaliaram-se as perdas em grãos armazenados em dois silos sob diferentes condições para conservação dos grãos: aeração convencional e refrigeração artificial. As amostragens foram feitas no centro e nas extremidades de cada silo sempre na superfície (0 a 5 m de profundidade). A cada 20 dias, durante três meses de armazenagem, foram determinados o teor de água, a massa específica aparente e a condutividade elétrica da solução dos exsudatos dos grãos. Observou-se, durante o período de armazenamento que, de modo geral, houve redução do teor de água e da massa específica aparente e aumento da condutividade elétrica da solução dos exsudatos dos grãos de soja armazenados nos dois silos independentemente da posição de coleta das amostras indicando que houve perdas quantitativas e uma piora na qualidade em ambas as condições. Porém, quando comparados os grãos dos dois tratamentos, as perdas foram menos acentuadas no silo sob refrigeração artificial. | EN: The objective of this work was to evaluate qualitative and quantitative losses during the soybeans storage period. The soybean used on this work was from producers from Sorriso-MT area and it was stored in the same town. We evaluate the losses in grains in two conditions of grains conservation: aeration with natural air and artificial refrigeration. Samplings were collected at the center and ends of each silo always in a surface (0 to 5 m of depth). Each 20 days, during three months of storage we determined the moisture content, bulk density and electrical conductivity of grains exudes. It was observed, during this storage period, that generally, the moisture content and bulk density reduced, and electrical conductivity of grains exudes increased, in both silos evaluated independently of the collection position, indicating quantitative losses and a worsening in quality in the two silos. However, when the grains in both silos are compared, the losses were less severe in the silo under refrigeration.
Thesagro: | Armazenamento; Glycine max; Qualidade.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/172349/1/2017-cpamt-silvia-botelho-perda-graos-soja-armazenado.pdf
Registro original: | Embrapa Agrossilvipastoril (CPAMT)
Exemplares: | CPAMT - (977-1) - UPC - AA - DD -  -  -  - DIS