Data/hora: 14/06/2024 02:27:19

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	23/06/2021	
Data da última atualização: 	10/06/2022	
Autoria: 	CONTI, P. P.; ANDRÉ, R. S.; MERCANTE, L. A.; FUGIKAWA-SANTOS, L.; CORREA, D. S.	
Afiliação: 	DANIEL SOUZA CORREA, CNPDIA.	
Título: 	Discriminative detection of volatile organic compounds using an electronic nose based on TiO2 hybrid nanostructures.	
Ano de publicação: 	2021	
Fonte/Imprenta: 	Sensors and Actuators: B. Chemical, v. 344, e130124, 2021.	
ISSN: 	0925-4005	
DOI: 	https://doi.org/10.1016/j.snb.2021.130124	
Idioma: 	Inglês	
Conteúdo: 	Volatile organic compounds (VOCs) are environmental pollutants that pose risks to the human health even at very low concentrations. Therefore, fast and sensitive analytical methods capable to discriminate VOCs are highly demanded. Herein, we have successfully synthetized and characterized TiO2 nanofibers (NF) by electrospinning and TiO2 nanoparticles (NP) by sol-gel method to be employed in an electronic nose (e-nose) for monitoring VOCs. Electrical comparison between TiO2-NF and TiO2-NP indicated that the former presented better electrical response, which can be attributed to the better charge transfer along the nanofiber framework. The TiO2 nanostructures were combined with three different polymers, namely poly(3,4- ethylenedioxythiophene):polystyrene sulfonate (PEDOT:PSS), polypyrrole (PPy), and polystyrene sulfonate (PSS), which obtained nanocomposites were deposit by drop casting onto gold interdigitated electrodes and used as sensing units of the e-nose. Electrical impedance spectroscopy measurements were employed to collect the enose electrical resistance data, which were treated by Principal Component Analysis (PCA), revealing the system was able to discriminate the three VOCs. Our results indicate that the e-nose system has potential to be employed as a rapid and simple alternative in the detection of VOCs.	
Palavras-Chave: 	E-nose; TiO2 nanofibers; TiO2 nanoparticles; VOCs sensor.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (17806-1) - UPC - AP - DD - PROCI.21/62 -  - 2021/62 - DIS