Data/hora: 22/09/2024 23:06:24

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	20/06/2022	
Data da última atualização: 	23/01/2024	
Autoria: 	PRADO, T. M. do; CATUNDA, L. G. S.; CORREA, D. S.; MACHADO, S. A. S.	
Afiliação: 	DANIEL SOUZA CORREA, CNPDIA.	
Título: 	Homemade Silver/Silver chloride ink with low curing temperature for screen-printed electrodes.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Journal of Electroanalytical Chemistry, v. 915, 116316, 2022.	
Páginas: 	6 p.	
ISSN: 	1572-6657	
DOI: 	https://doi.org/10.1016/j.jelechem.2022.116316	
Idioma: 	Inglês	
Conteúdo: 	Here we report the synthesis of Ag/AgCl ink with low curing temperature for application in electrochemical sensors. The ink characterization was carried out by atomic force microscopy, scanning electron microscopy with energy dispersive spectroscopy, X-ray diffraction, thermogravimetry analysis, DC electrical resistivity, and cyclic voltammetry. Furthermore, the ink was used in a pseudo reference electrode of a screen-printed device, which was then applied for carbendazim quantification as proof of concept. The electrochemical sensor presented linear response in the range of carbendazim concentrations from 0.25 to 1.48 µmol L&#8722;1 and limit of detection of 0.10 µmol L&#8722;1, suggesting the potential of the as-developed ink for designing miniaturized electrochemical sensing devices	
Palavras-Chave: 	Electroanalysis; Miniaturized device; Screen printed electrode; Silver ink.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (18031-1) - UPC - AP - DD - PROCI.22/73 -  - 2022/80 - DIS