Data/hora: 09/06/2024 13:47:53

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	30/03/2006	
Data da última atualização: 	30/03/2006	
Autoria: 	APPOLONI, C. R.; MACEDO, A.; FERNANDES, C. P.; PHILIPPI, P. C.	
Título: 	Characterization of porous microstructure by X-ray microtomography.	
Ano de publicação: 	2000	
Fonte/Imprenta: 	In: SEMINÁRIO LATINO-AMERICANO DE ANÁLISES POR TÉCNICAS DE RAIOS X - SARX 2000, 7., São Pedro. [Abstracts...]. Campinas: Oficinas Gráficas da Universidade Estadual de Campinas, 2000. p.179, ref. RT-03.	
Idioma: 	Inglês	
Conteúdo: 	Present work deals with the measurement of microstructural parameters of petroleum reservoir rocks and porous ceramic filters. Microtomographic measurements of samples were performed by employing an X-ray tube with W anode, at 70 kV and 10mA.	
Palavras-Chave: 	Microtomography; Porous materials.	
Thesaurus Nal: 	microstructure.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9699-1) - UPC - SP - -- - PROCI-00.00006 -  - 2000.00006 - DIS