Data/hora: 03/06/2024 04:54:28

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	16/03/2022	
Data da última atualização: 	16/03/2022	
Autoria: 	AGUIAR, L. M. de; GALVAN, D.; BONA, E.; COLNAGO, L. A.; KILLNER, M. H. M.	
Afiliação: 	LUIZ ALBERTO COLNAGO, CNPDIA.	
Título: 	Data fusion of middle-resolution NMR spectroscopy and low-field relaxometry using the Common Dimensions Analysis (ComDim) to monitor diesel fuel adulteration.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Talanta, v. 236, 122838, 2022.	
Páginas: 	1 - 10	
ISSN: 	0039-9140	
DOI: 	https://doi.org/10.1016/j.talanta.2021.122838	
Idioma: 	Inglês	
Conteúdo: 	Medium-resolution (MR-NMR) and time-domain NMR relaxometry (TD-NMR) using benchtop and low-field NMR instruments are powerful tools to tackle fuel adulteration issues. In this work, for the first time, we investigate the possibility of enhancing the low-field NMR capability on fuel analysis using data fusion of MR and TD-NMR. We used the ComDim (Common Dimensions Analysis) multi-block analysis to join the data, which allowed exploration, classification, and quantification of common adulterations of diesel fuel by vegetable oils, biodiesel, and diesel of different sources as well as the sulfur content. After data exploration using ComDim, classification (applying linear discriminant analysis, LDA), and regression (applying multiple linear regression, MLR), models were built using ComDim scores as input variables on the LDA and MLR analyses. This approach enabled 100% of accuracy in classifying diesel fuel source (refinery), sulfur content (S10 or S500), vegetable oil, and biodiesel source. Moreover, in the quantification step, all MLR models showed a root mean square error of prediction (RMSEP) and the residual prediction deviation (RPD) values comparable to the literature for determining diesel, vegetable oil, and biodiesel contents.	
Palavras-Chave: 	Linear discriminant analysis; Low-field proton nuclear magnetic resonance; Multi-block analysis; Multiple linear regression.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (17934-1) - UPC - AP - DD - PROCI.22/05 -  - 2022/05 - DIS