Data/hora: 09/06/2024 01:26:29

Biblioteca(s): 	Embrapa Meio Ambiente.	
Data corrente: 	21/01/2020	
Data da última atualização: 	21/01/2020	
Autoria: 	VICENTE, L. E.; LOEBMANN, D. G. dos S. W.; PAZIANOTTO, R. A. A.; FAGGIONI, M.; GOMES, A. C. C.	
Afiliação: 	LUIZ EDUARDO VICENTE, CNPMA; DANIEL GOMES DOS SANTOS W LOEBMANN, CNPMA; RICARDO ANTONIO ALMEIDA PAZIANOTTO, CNPMA; MIGUEL FAGGIONI, UNICAMP; ANA CAROLINA CAMPOS GOMES.	
Título: 	SCAI-r: an algorithm for obtaining synoptic and spatial atmospheric parameters.	
Ano de publicação: 	2019	
Fonte/Imprenta: 	In: SIMPÓSIO BRASILEIRO DE SENSORIAMENTO REMOTO, 19., 2019, Santos. Anais... São José dos Campos: INPE, 2019. Ref. 96399.	
Páginas: 	p. 1-4.	
ISBN: 	978-85-17-00097-3	
Idioma: 	Inglês	
Conteúdo: 	Abstract: The highest performance of multiband optical data (Visible - VIS ? Shortwave Infrared - SWIR ? (400-2500 nm) (e.g. imaging spectroscopy approaches) can be reached mainly through atmospheric correction effects; the conversion of the image values to surface reflectance, allowing, for instance, to estimate the amount of biochemical compounds in the target. This work aims to present an algorithm dedicated to atmospheric parameters obtaining from MODIS and related sensors, encapsulated in a user-friendly interface through Software to Collect Atmospheric Information (SCAI-r), applied to the correction of atmosphere effects on Rapideye image. The results show that SCAI-r generates information needed to perform atmospheric correction and that it has a greater influence over water-related objects, when compared to parameters randomly inserted as input data in atmospheric correction algorithms.	
Palavras-Chave: 	Aerosol Optical Thickness; Atmospheric Correction; Radiative Transfer Model; RapidEye; Visibility.	
Thesagro: 	Satélite; Sensoriamento Remoto.	
Thesaurus Nal: 	Radiative transfer; Remote sensing.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/209287/1/Vicente-scai-algorithm-2019.pdf	
Registro original: 	Embrapa Meio Ambiente (CNPMA)	
Exemplares: 	CNPMA - (16699-1) - UPC - AA - DD -  -  -  - DIS