Data/hora: 22/06/2024 00:20:44

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 28/03/2005
Data da última atualização: | 28/03/2005
Autoria: | MORENO, R. M. B.; MEDEIROS, E. S.; FERREIRA, F. C.; ALVES, N.; GONÇALVES, P. S.; MATTOSO, L. H. C.
Título: | Estudo da cinética de decomposição de quatro clones de seringueira utilizando o método de ozawa.
Ano de publicação: | 2003
Fonte/Imprenta: | In: CONGRESSO BRASILEIRO DE POLÍMEROS. 7., nov. 2003., Belo Horizonte, MG. Anais... São Carlos: Associação Brasileira de Polímeros, 2003. p. 1007-1008.
Idioma: | Português
Conteúdo: | Thermal degradation behavior of rubber from four rubber clones (RRIM 600, PB 235, GT1 and IAN 873) of the Hevea brasiliensis species was studied by thermogravimetry (TG) using Ozawa?s approach to assess the kinetic parameters of the decomposition process. The order of reaction follows zero-order kinetic at the beginning and the end of the degradation process, and first order at intermediate stages. Activation energy were determined to be dependent on the degree of conversion and clone used ragging from 148 to 236kJ/mol. These values indicated that the thermal behavior of natural rubber depends on the type of clones studied. Rubber from clones IAN 873, GT1 and RRIM 600 presented the best overall thermal stability whereas the clone PB 235 presented a lower thermal stability than for any other clone studied.
Palavras-Chave: | Comportamento térmico; Polímeros.
Thesagro: | Latex.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (8761-1) - UPC - SP - -- - PROCI-03.00106 -  - 2003.00106 - DIS