Data/hora: 11/06/2024 17:57:50

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 27/03/2006
Data da última atualização: | 27/03/2006
Autoria: | VAZ, C. M. P.; HOPMANS, J. W.
Título: | TDR probes for combined use with a cone penetrometer to determine water content influence on soil strength.
Ano de publicação: | 1999
Fonte/Imprenta: | In: AMERICAN SOCIETY OF AGRONOMY ANNUAL MEETING, 91., 1999, Salt Lake City. 1999 Annual meeting abstracts... New York: ASA: CSSA: SSSA, 1999. p.193.
Idioma: | Inglês
Conteúdo: | Soil mechanical impedance affects root growth and water flow, and controls nutrient and contaminant transport below the rooting zone. Among the soil parameters affecting soil strength, soil water content and bulk density are the most significant. However, field water content changes both spatially and temporally, limiting the application of penetrometers as an indicator of soil strength.
Palavras-Chave: | Penetrometer; TDR.
Thesaurus Nal: | impedance; soil.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9671-1) - UPC - SP - -- - PROCI-99.00149 -  - 1999.00149 - DIS