Data/hora: 23/09/2024 04:53:08

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	28/03/2006	
Data da última atualização: 	28/03/2006	
Autoria: 	VASQUES, R. A.; INNOCENTINI, M. D. M.; ASSIS, O. B. G.	
Título: 	A simple apparatus for determining the permeability of thin-thickness porous materials by pressure-decay technique.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	Revista de Física Aplicada e Instrumentação, Rio de Janeiro, v.14, n.4, p.120-123, dez. 1999.	
Idioma: 	Inglês	
Conteúdo: 	A simple experimental set up, for the evaluation of the permeability of thin-thickness porous material, is presented. The proposed system makes use of a perpendicular fluid flux that at controlled pressure can permeate the medium.The permeability variables are estimated by measuring the relative pressure before and after the fluid permeates the sample.	
Palavras-Chave: 	Materiais porosos; Membranas vítreas.	
Thesagro: 	Permeabilidade.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9679-1) - UPC - SP - -- - PROCI-99.00155 -  - 1999.00155 - DIS