Data/hora: 24/06/2024 19:13:12

Biblioteca(s): 	Embrapa Solos.	
Data corrente: 	17/12/2019	
Data da última atualização: 	27/04/2022	
Autoria: 	KOTLAR, A. M.; LIER, Q. de J. van; BARROS, A. H. C.; IVERSEN, B. V.; VEREECKEN, H.	
Afiliação: 	ALI MEHMANDOOST KOTLAR, CENA/USP; QUIRIJN DE JONG VAN LIER, CENA/USP; ALEXANDRE HUGO CEZAR BARROS, CNPS; BO V. IVERSEN, AARHUS UNIV., DENMARK; HARRY VEREECKEN, INSTITUTE OF BIO- AND GEOSCIENCES (IBG-3), AGROSPHERE, FORSCHUNGSZENTRUM JULICH, GERMANY.	
Título: 	Development and uncertainty assessment of pedotransfer functions for predicting water contents at specific pressure heads.	
Ano de publicação: 	2019	
Fonte/Imprenta: 	Vadose Zone Journal, v. 18, n. 1, 190063, 2019.	
DOI: 	10.2136/vzj2019.06.0063	
Idioma: 	Inglês	
Conteúdo: 	There has been much effort to improve the performance of pedotransfer functions (PTFs) using intelligent algorithms, but the issue of covariate shift, i.e., different probability distributions in training and testing datasets, and its impact on prediction uncertainty of PTFs has been rarely addressed. The common practice in PTF generation is to randomly separate the dataset into training and testing subsets, and the outcomes of this random selection may be different if the process is subject to covariate shift. We evaluated the impact of covariate shift generated by data shuffling and detected by Kolmogorov-Smirnov test for the prediction of water contents using soil databases from Denmark and Brazil. The soil water contents at different pressure heads were predicted by developing linear and stepwise regression besides machine learning based PTFs including Gaussian process regression and ensemble method. Regression based PTFs for the Brazilian dataset resulted in better predictions compared with machine learning methods, which in their turn estimated high water contents in Danish soils more accurately. One hundred PTFs were developed for water content at specific pressure heads by data shuffling. From these, 100 sets of fitted van Genuchten parameters were obtained representing the generated uncertainty. Data shuffling led to covariate shift, resulting in uncertainty in water content prediction by the PTFs. Inherent variability of data may lead to increased prediction uncertainty. For correlated data, simple regression models performed as good as sophisticated machine learning methods. Using PTF-predicted water contents for van Genuchten retention parameter fitting may lead to a high uncertainty.	
Palavras-Chave: 	Funções de pedotransferência.	
Thesagro: 	Condutividade Hidráulica; Retenção de Água no Solo.	
Thesaurus Nal: 	Hydraulic conductivity; Pedotransfer functions; Soil water retention.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/207273/1/Development-and-uncertainty-assessment-of-pedotransfer-functions-2019.pdf	
Registro original: 	Embrapa Solos (CNPS)	
Exemplares: 	CNPS - (20377-1) - UPC - AP - DD -  -  - 2019.00285 - DIS