Data/hora: 12/06/2024 22:01:05

Biblioteca(s): 	Embrapa Agricultura Digital.	
Data corrente: 	27/05/1996	
Data da última atualização: 	17/08/2007	
Autoria: 	BARROS, I. M.; LOTUFO, R de A.; LEITE, N. J.	
Título: 	Arquitetura VLSI de operacoes de morfologia matematica.	
Ano de publicação: 	1994	
Fonte/Imprenta: 	In: SEMINÁRIO INTEGRADO DE SOFTWARE E HARDWARE, 21., 1994, Caxambu. Anais... Belo Horizonte: UFMG, 1994.	
Páginas: 	p.55-66	
Idioma: 	Inglês	
Conteúdo: 	This paper presents a sistolic architeture for the realization of non-linear filters (mathematical morphological filters) on both binary and gray-level images. Due to its regularity and modularity, it is well suited for VLSI implementation. This architeture is suitable for dilation and erosion operation with a planar structuring element, in binary and numerical modes of operation, with the macimum exploration of the hardware on both models. The simulation of this architecture is made through the hardware description language VHDL. Structural comparisons between this architecture and others are also made, showing its superiority.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Agricultura Digital (CNPTIA)	
Exemplares: 	CNPTIA - (3148-1) - ADD - PL - -- - 004 - SEM - 1996.00003 - DIS