Data/hora: 05/06/2024 11:13:15

Biblioteca(s): | Embrapa Clima Temperado; Embrapa Instrumentação.
Data corrente: | 04/03/2024
Data da última atualização: | 08/04/2024
Autoria: | AVILA, L. O. de; TORRES, D. P.; ORESTE, E. Q.; LISBOA, M. T.; SILVEIRA, C. A. P.; RIBEIRO, A. S.; NUNES, A. M.; MARTINAZZO, R.
Afiliação: | LIZIANE OLIVEIRA DE AVILA, UNIVERSIDADE FEDERAL DE PELOTAS; DAIANE PLACIDO TORRES, CNPDIA; ELIÉZER QUADRO ORESTE, UNIVERSIDADE FEDERAL DO RIO GRANDE; MEIBEL TEIXEIRA LISBOA, UNIVERSIDADE FEDERAL DE PELOTAS; CARLOS AUGUSTO POSSER SILVEIRA, CPACT; ANDERSON SCHWINGEL RIBEIRO, UNIVERSIDADE FEDERAL DE PELOTAS; ADRIANE MEDEIROS NUNES, UNIVERSIDADE FEDERAL DE PELOTAS; ROSANE MARTINAZZO, CPACT.
Título: | Speciation of Inorganic Arsenic in Retorted Oil Shale Slurry by Hydride Generation Atomic Absorption Spectrometry (HG AAS) after Ultrasound-Assisted Acid Extraction.
Ano de publicação: | 2024
Fonte/Imprenta: | Analytical Letters, v. 57, n. 7, p. 1065-1077, 2024.
DOI: | https://doi.org/10.1080/00032719.2023.2240453
Idioma: | Inglês
Conteúdo: | An analytical method for determination of inorganic arsenic speciesin retorted oil shale slurry by atomic absorption spectrometrycoupled to hydride technique with ultrasound assisted acidic extrac-tion is reported. Trivalent arsenic measurement employed samplestabilization with a pH 4.5 prior to reaction with the reducing agentand analysis. In contrast, total inorganic As depended upon the pre-reduction of As(V) to As(III) with KI and ascorbic acid in 6.0 M HCland of As(V) was estimated by the difference of the total inorganicAs and As(III) concentrations. The limit of quantification was 3.7 mgkg1for As(III) and 1.3 mg kg1for itAs
Thesagro: | Arsênico; Espectrometria; Rocha; Xisto.
Thesaurus Nal: | Shale.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)

Exemplares:

CPACT - (22798-1) - UPC - AP - DD -  -  -  - DIS
CNPDIA - (18404-1) - UPC - AP - DD - PROCI.24/23 -  - 2024/28 - DIS