Data/hora: 21/09/2024 09:06:48

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	23/01/2006	
Data da última atualização: 	23/01/2006	
Autoria: 	MEDEIROS, E. S. de; AGNELLI, J. A. M.; JOSEPH, K.; CARVALHO, L. H. De. MATTOSO, L. H. C.	
Título: 	Mechanical properties of phenolic composites reinforced with jute/cotton hybrid fabrics.	
Ano de publicação: 	2006	
Fonte/Imprenta: 	Polymer composites, Brookfield, v.26, n. 1, Feb. 2005. Disponível em: <http://dx.doi.org/10.1002/pc.20063>. Acesso em: 6 jan. 2006.	
Idioma: 	Inglês	
Conteúdo: 	Mechanical properties (tensile, flexural, impact, and dynamic mechanical thermal analysis) of novolac type phenolic composites reinforced with jute/cotton hybrid woven fabrics were investigated as a function of fiber orientation and roving/fabric characteristics. Scanning electron microscopy (SEM) was carried out to investigate the fiber-matrix adhesion. Results showed that the composite properties are strongly influenced by test direction and rovings/fabric characteristics.	
Palavras-Chave: 	Fiber-matrix; Scaning electron microscopy; SEM.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9224-1) - UPC - SP - -- - PROCI-05.00067 -  - 2005.00067 - DIS