Data/hora: 21/06/2024 05:44:31

Biblioteca(s): 	Embrapa Gado de Leite.	
Data corrente: 	31/08/2018	
Data da última atualização: 	24/01/2023	
Autoria: 	MENDONÇA, H. V. de; OMETTO, J. P. H. B.; OTENIO, M. H.; MARQUES, I. P. R.; REIS, A. J. D. dos.	
Afiliação: 	Henrique Vieira de Mendonça, UFJF; Jean Pierre Henry Balbaud Ometto, INPE; MARCELO HENRIQUE OTENIO, CNPGL; Isabel Paula Ramos Marques, National Laboratory of Energy and Geology, Lisbon, Portugal; Alberto José Delgado dos Reis, National Laboratory of Energy and Geology, Lisbon, Portugal.	
Título: 	Microalgae-mediated bioremediation and valorization of cattle wastewater previously digested in a hybrid anaerobic reactor using a photobioreactor: Comparison between batch and continuous operation.	
Ano de publicação: 	2018	
Fonte/Imprenta: 	Science of The Total Environment, v. 633, p. 1-11, 2018.	
Idioma: 	Inglês	
Conteúdo: 	Abstract Scenedesmus obliquus (ACOI 204/07) microalgae were cultivated in cattle wastewater in vertical alveolar flat panel photobioreactors, operated in batch and continuous mode, after previous digestion in a hybrid anaerobic reactor. In batch operation, removal efficiencies ranges of 65 to 70% of COD, 98 to 99% of NH4+ and 69 to 77.5% of PO4-3 after 12days were recorded. The corresponding figures for continuous flow were from 57 to 61% of COD, 94 to 96% of NH4+ and 65 to 70% of PO4-3 with mean hidraulic retention time of 12days. Higher rates of CO2 fixation (327-547mgL-1d-1) and higher biomass volumetric productivity (213-358mgL-1d-1) were obtained in batch mode. This microalgae-mediated process can be considered promising for bioremediation and valorization of effluents produced by cattle breeding yielding a protein-rich microalgal biomass that could be eventually used as cattle feed.	
Palavras-Chave: 	Cattle wastewater; CO(2) fixation; Flat panel photobioreactor; Nutrient removal.	
Thesagro: 	Microalga.	
Thesaurus Nal: 	Microalgae.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (24101-1) - UPC - AP - DD -  -  -  - DIS