Data/hora: 23/06/2024 04:22:23

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 02/03/2006
Data da última atualização: | 20/06/2018
Autoria: | CRUVINEL, P. E.; VIEIRA, S. R.; CRESTANA, S.; MINATEL, E. R.; MUCHERONI, M. L.; TORRE-NETO, A.
Título: | Image processing in automated measurements of raindrop size and distribution.
Ano de publicação: | 1999
Fonte/Imprenta: | Computers and Electronics in Agriculture, Amsterdam, v.23, p.205-217, 1999.
Volume: | 23
Páginas: | 205-217
DOI: | https://doi.org/10.1016/S0168-1699(99)00043-5
Idioma: | Inglês
Conteúdo: | A rapid method for evaluating raindrop size and size distribution has been developed. It is based on image processing with correlation analysis in the frequency domain. This technique has the advantage of being a direct measurement method that automatically identifies and counts raindrops.
Palavras-Chave: | Correlation analysis; Raindrop measurements.
Thesaurus Nal: | soil conservation.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9499-1) - UPC - SP - -- - PROCI-99.00050 -  - 1999.00050 - DIS