Data/hora: 23/06/2024 07:04:19

Biblioteca(s): | Embrapa Mandioca e Fruticultura.
Data corrente: | 15/09/2000
Data da última atualização: | 15/09/2000
Autoria: | LUTZ, K.; MUHLBAUER, W.; MULLER, J.; REISINGER, G.
Afiliação: | Institute for Agricultural Engineering, Hohenheim University, 7000 Stuttgart 70, Garbenstasse 9, Federal Republic of Germany.
Título: | Development of a multi-purpose solar crop dryer for arid zones.
Ano de publicação: | 1987
Fonte/Imprenta: | Solar and Wind Technology, v.4, p.417-424, 1987.
Idioma: | Inglês
Conteúdo: | A multi purpose solar crop dryer was developed for drying various agricultural products such as fruits, vegetables, medicinal plants etc. The newly developed system consists of a small fan, a solar air heater and a tunnel dryer. The simple desing allows productions either by farmers themselves, using cheap and locally available materials, or by small scale industries. Due to the low investment required, the solar dryer is predestined for application on small farms in developing countrines. Depending on the crop to be dried and the size of the dryer 100-1000 kg of fresh material can be dried within 1-7 days to safe storange conditions. The solar dryer was successfully tested in Greece, Yugoslavia.
Palavras-Chave: | Aspecto economico; Secagem solar.
Thesagro: | Alimento; Energia Solar.
Categoria do assunto: | --
Registro original: | Embrapa Mandioca e Fruticultura (CNPMF)
Exemplares: | CNPMF - (15367-1) - ADC - SP - -- - S1460 -  - S1460 - DIS