Data/hora: 23/06/2024 18:38:56

Biblioteca(s): | Embrapa Agricultura Digital.
Data corrente: | 08/08/1996
Data da última atualização: | 27/02/2013
Autoria: | FRERY, A. C.; SANT'ANNA, S. J. S.
Afiliação: | ALEJANDRO C. FRERY, INPE; SIDNEI J. S. SANT'ANNA, INPE.
Título: | Non-adaptive robust filters for speckle noise reduction.
Ano de publicação: | 1993
Fonte/Imprenta: | In: SIMPÓSIO BRASILEIRO DE COMPUTAÇÃO GRÁFICA E PROCESSAMENTO DE IMAGENS, 6., 1993, Recife. Anais... Recife: SBC: UFPe, 1993.
Páginas: | p. 165-174.
Idioma: | Inglês
Notas: | Evento conhecido como SIBGRAPI. Editado por Luiz H. de Figueiredo e Jonas de Miranda Gomes.
Conteúdo: | After briefly reviwing some classical filters for speckle removal, five filters with characteristics of robustness, suitable for speckle noise reduction, are derived and implemented. These filters are the ones based on the trimmed maximum likelihood and moments estimators, the one based on the median, on the inter-quartile range and on the median absolute deviation. Assuming that observations within a synthetic aperture radar image are outcomes of independent Rayleigh random variables, these filters exhibit a good performance from both the signal-to-noise reduction and from the edge preserving criteria. The problem of filtering in an image is posed as an estimation problem.
Thesagro: | Estatística; Estimativa.
Thesaurus Nal: | Estimation; Statistics.
Categoria do assunto: | X Pesquisa, Tecnologia e Engenharia
Registro original: | Embrapa Agricultura Digital (CNPTIA)
Exemplares: | CNPTIA - (3775-1) - ADD - PL - PP - 006.6 - SIM - 1994.00004 - DIS