Data/hora: 23/09/2024 11:57:48

Biblioteca(s): 	Embrapa Solos.	
Data corrente: 	14/02/2022	
Data da última atualização: 	24/02/2022	
Autoria: 	VASQUES, G. de M.; RODRIGUES, H. M.; HUBER, E.; TAVARES, S. R. de L.; MARQUES, F. A.; SILVA, M. S. L. da.	
Afiliação: 	GUSTAVO DE MATTOS VASQUES, CNPS; HUGO MACHADO RODRIGUES, UFRRJ; EMANUEL HUBER, GEOTEST Ltd.; SILVIO ROBERTO DE LUCENA TAVARES, CNPS; FLAVIO ADRIANO MARQUES, CNPS; MARIA SONIA LOPES DA SILVA, CNPS.	
Título: 	Ground penetrating radar non-invasively positions an underground dam and estimates its water reservoir shape and volume.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	In: PEDOMETRICS BRAZIL, 2., 2021, Rio de Janeiro. Annals [...]. Rio de Janeiro: Embrapa Solos, 2022. Não paginado. Evento online.	
Idioma: 	Inglês	
Conteúdo: 	The objectives are to use ground penetrating radar (GPR) to: (a) find a suitable length and location for a future underground dam; and (b) model the shape and estimate the volume of its water reservoir. Radargrams were obtained in a 0.85-ha area in northeastern Brazil along five survey lines parallel to, and eight lines transverse to the slope, starting from the proposed location of the dam. The 13 radargrams were pre-processed and migrated. The terrain surface and the top of the regolith delineated in the radargrams were interpolated, plotted in 3D showing the shape of the water reservoir, and used to estimate its volume. From the radargrams, the future dam should be 45 m longer and centered 22 m south of the proposed location, increasing the water reservoir by 50% to a total of 6 million L. By assessing the terrain surface and regolith, the GPR allows to adjust the length and position future underground dams and assess their water reservoir shape and volume non-invasively.	
Palavras-Chave: 	Brazilian semiarid region; GPR.	
Thesagro: 	Barragem Subterrânea; Radar; Solo.	
Thesaurus Nal: 	Geophysics; Regolith; Soil depth.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/231289/1/Ground-penetrating-radar-non-invasively-positions-2022.pdf	
Registro original: 	Embrapa Solos (CNPS)	
Exemplares: 	CNPS - (21002-1) - UPC - AA - DD -  -  -  - DIS