Data/hora: 22/06/2024 03:39:49

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 27/03/2006
Data da última atualização: | 27/03/2006
Autoria: | SIMÕES, M.; ASSIS, O. B. G.; AVACA, L. A.
Título: | Electrochemical characterization of sol-gel protective ZrO2 coatings on sintered stainless steels.
Ano de publicação: | 1999
Fonte/Imprenta: | In: INTERNATIONAL LATIN-AMERICAN CONFERENCE ON POWDER TEHNOLOGY-PTECH, 2., 1999, Foz do Iguaçu. PTECH'99: powder technology: challenges for the next millenium. [S. l.]: Associação Brasileira de Cerâmica, 1999. Não-paginado, ref. MO88.
Idioma: | Inglês
Conteúdo: | ZrO2 films derived from Sol-Gel technique were obtained by dip-coatings onto commercial sintered AlSi 304 and 316 stainless steel compositions. The coatings were processed from a sirconium (4) propoxide precursor solution, sinterized at 800 °C for 2 hours in air.
Palavras-Chave: | Electrochemical corrosion; Passive coating; Sol-gel; Surface analysis.
Thesaurus Nal: | microscopy.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9661-1) - UPC - SP - -- - PROCI-99.00141 -  - 1999.00141 - DIS