Data/hora: 23/05/2024 15:03:25

Biblioteca(s): 	Embrapa Gado de Corte.	
Data corrente: 	21/02/2011	
Data da última atualização: 	25/02/2011	
Autoria: 	COELHO, M. de B.; CARVALHO, J. A.; FERREIRA, V. S.; ARAUJO, F. R.; SOARES, C. O.; HERRMANN JUNIOR, P. S. de P.; MARCONCINI, J. M.	
Afiliação: 	MARLENE DE BARROS COELHO, CNPGC; UFMS; UFMS; FLABIO RIBEIRO ARAUJO, CNPGC; CLEBER OLIVEIRA SOARES, CNPGC; PAULO SERGIO DE P HERRMANN JUNIOR, CNPDIA; JOSE MANOEL MARCONCINI, CNPDIA.	
Título: 	Nanostructured screen-printed electrodes for immunosensor.	
Ano de publicação: 	2010	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON FOOD AND AGRICULTURE APPLICATIONS OF NANOTECHNOLOGIES - NanoAgri, 2010, São Pedro, SP. [Anais?] São Pedro: Aptor Software, 2010. Editors: Caue Ribeiro, Odílio Benedito Garrido de Assis, Luiz Henrique Capparelli Mattoso, Sérgio Mascarenhas.	
Páginas: 	1 p.	
Idioma: 	Inglês	
Conteúdo: 	Gold nanoparticles have been distributed by chemisorption interaction in a three dimensional structure of MTMPS sol-gel. This novel feature of modified electrodes has been mounted on screen-printed gold electrodes and it is being used to detect biomolecules interactions. Through a small variation of an electrical signal under the modified electrode one can build a model that describes a specific antigen-antibody binding. Electrochemistry impedance spectroscopy has found to be an effective analysis that transduces this electrical signal. In the present work, we have been exploiting these three concepts to create an innovative method for
diagnosis of important bovine diseases by immunoassay.	
Palavras-Chave: 	Imunosensor; Nanotecnologia.	
Thesagro: 	Sanidade Animal.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Gado de Corte (CNPGC)	
Exemplares: 	CNPGC - (13760-1) - UPC - SP - PP -  -  - 002/20 - DIS