Data/hora: 22/06/2024 08:22:18

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	29/05/2003	
Data da última atualização: 	31/07/2009	
Autoria: 	AZEREDO, R. B.; COELHO, I.; TAVARES, M. I. B.; ENGELSBERG, M.; COLNAGO, L. A.	
Afiliação: 	Embrapa Instrumentação Agropecuária, São Carlos, SP; Instituto de Química de São Carlos-USP, São Carlos, SP; Faculdade de Odontologia-USP; Instituto de Macromoléculas-UFRJ; Departamento de Física-UFPE, Recife.	
Título: 	Analysis of the photopolymerization rate of methacrylate blends by continuous wave free precession NMR.	
Ano de publicação: 	2003	
Fonte/Imprenta: 	In: ENCONTRO DE USUÁRIOS DE RESSONÂNCIA MAGNÉTICA NUCLEAR, 9., 2003, Angra dos Reis. Extended abstracts... Angra dos Reis> AUREMN, 2003.	
Idioma: 	Português	
Conteúdo: 	Here we used the continuous wave free precession (CWFP)2 technique to analyze the photopolymerization rate of the dimethacrylate blends with milisecond time resolution in the CWFP experiments a trains for pulses separated by a time interval Tr, shorter han T2, is used.	
Palavras-Chave: 	CWFP; Dimethacrylate.	
Thesaurus Nal: 	polymerization.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (7529-1) - UPC - SP - -- - PROCI-03.00010 -  - 2003.00010 - DIS