Data/hora: 04/06/2024 01:54:11

Biblioteca(s): | Embrapa Agroenergia.
Data corrente: | 21/07/2022
Data da última atualização: | 21/07/2022
Autoria: | HUNT, J. D.; NASCIMENTO, A.; GUZMAN, O. J. R.; FURTADO, G. C. de A.; CATEN, C. S. T.; TOMÉ, F. M. C.; LEAL FILHO, W.; DURIN, B.; LOPES, M. A.; WADA, Y.
Afiliação: | JULIAN DAVID HUNT, Universidade Federal do Espírito Santo; ANDREAS NASCIMENTO, Universidade Federal do Espírito Santo; OLDRICH JOEL ROMERO GUZMAN, Universidade Federal do Espírito Santo; GILTON CARLOS DE ANDRADE FURTADO, Universidade Federal do Pará; CARLA SCHWENGBER TEN CATEN, Universidade Federal do Rio Grande do Sul; FERNANDA MUNARI CAPUTO TOMÉ, Universidade De São Paulo; WALTER LEAL FILHO, Universidade de Ciências Aplicadas de Hamburg, Alemanha; BOJAN ÐURIN, University North, Varaždin, Croácia; MAURICIO ANTONIO LOPES, CNPAE; YOSHIHIDE WADA, Instituto Internacional de Análise de Sistemas Aplicados, Laxenburg, Áustria.
Título: | Sedimentary BasinWater and Energy Storage: a low environmental impact option for the bananal basin.
Ano de publicação: | 2022
Fonte/Imprenta: | Energies, 15, n. 4498, 2022.
DOI: | https://doi.org/10.3390/en15124498
Idioma: | Inglês
Conteúdo: | Groundwater storage is an important water management solution that is overlooked by several countries worldwide. This paper evaluates the potential for storing water in the Bananal sedimentary basin and proposes the construction of canals to reduce sediment obstructions in the river flow and harmful flood events. This would allow for better control of the water level. The water stored in the sedimentary basin can be used as a climate change adaptation measure to ensure that the level of the flood plain is maintained high during a drought or low during an intense flood event. Additionally, the flood plain will function as a water reservoir, regulate the river flow downstream from the flood plain, and enhance hydropower generation. A significantly smaller reservoir area is expected to store water, as the water will be stored as groundwater in the sedimentary basin. Results show that the Bananal basin has the potential to store up to 49 km3 of water, which can add up to 11.7 TWh of energy storage to the Brazilian energy matrix for a CAPEX energy storage cost of 0.095 USD/kWh. This is an interesting solution for the Araguaia basin and several other basins worldwide.
Palavras-Chave: | Energy storage; Hydropower; Renewable energies; Sedimentary basin.
Thesaurus Nal: | Water management.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1144869/1/Mauricio-.pdf
Registro original: | Embrapa Agroenergia (CNPAE)
Exemplares: | CNPAE - (4054-1) - UPC - AP - DD -  -  -  - DIS