Data/hora: 26/07/2024 22:41:41

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	26/08/2005	
Data da última atualização: 	26/08/2005	
Autoria: 	MALMONGE, J. A.; CAMPOLI, C. S.; MALMONGE, L. F.; KANDA, D. H. F.; MATTOSO, L. H. C.; CHIERICE, G. O.	
Título: 	Effect of the doping medium on blends of polyurethane and polyaniline.	
Ano de publicação: 	2001	
Fonte/Imprenta: 	Synthetic Metals, Amsterdam, v. 119, p. 87-88, 2001.	
Idioma: 	Inglês	
Conteúdo: 	Flexible and free-stantding films from blends of polyurethane, based on castor oil, and polyaniline were obtained with various compositions by casting. Significant increase on conductivity followed by a considerable decrease on doping time was obtained by doping the films in N, N-dimethylformamide (DMF) solution with p-toluene sulphonic acid (TSA) or HCl instead of the conventional doping aqueous solution. This doping efficiency is proposed to be due to an improved swelling of the blend structure caused by the solvent.	
Palavras-Chave: 	blends; doping; Polimeros condutores; polyanilina; polyurethane.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8934-1) - UPC - SP - -- - PROCI-01.00027 -  - 2001.00027 - DIS