Data/hora: 27/07/2024 02:36:53

Biblioteca(s): 	Embrapa Agrossilvipastoril.	
Data corrente: 	11/02/2019	
Data da última atualização: 	11/02/2019	
Autoria: 	HAUTH, M. R.; BOTELHO, F. M.; HOSCHER, R. H.; BOTELHO, S. de C. C.; OLIVEIRA, G. H. H. de.	
Afiliação: 	MICHELE R. HAUTH, UFGD; FERNANDO M. BOTELHO, UFMT, SINOP; RENATA H. HOSCHER, UFGD; SILVIA DE CARVALHO CAMPOS BOTELHO, CPAMT; GABRIEL H. H. DE OLIVEIRA, IFMG.	
Título: 	Physical properties of different soybean cultivars during drying.	
Ano de publicação: 	2018	
Fonte/Imprenta: 	Engenharia Agrícola, v. 38, n. 4, p. 590-598, 2018.	
ISSN: 	1809-4430	
DOI: 	http://dx.doi.org/10.1590/1809-4430-Eng.Agric.v38n4p590-598/2018	
Idioma: 	Inglês	
Conteúdo: 	The knowledge of physical properties of grains is important for the optimization of postharvest operations. Thus, this study aimed to evaluate the effect of moisture content over physical properties of different cultivars of soybean. Soybean of cultivars NS7901RR, TMG1180RR, P98Y70 and TMG132RR were used, with initial moisture content of 0.32, 0.27, 0.25 and 0.21 dry basis (d.b.), respectively. In order to dry the samples, an oven of forced air circulation was used. Samples were dried at temperature of 50 ºC, being the drying procedure stopped when the moisture content of soybean was equal or inferior than 0.15 (d.b.). During drying, for interested moisture contents, physical properties were determined: bulk density, equivalent diameter, sphericity, circularity and surface/volume ratio. It was noticed that all physical properties analyzed presented a direct relationship with moisture content. With exception of the equivalent diameter, all the remaining physical properties increased linearly with moisture content reduction. Physical differences were observed among soybean cultivars during drying. However, variation of analyzed properties occurred in different proportions during drying for each cultivar.	
Thesaurus Nal: 	Physical properties; Shape; Soybeans.	
Categoria do assunto: 	F Plantas e Produtos de Origem Vegetal	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/192508/1/2018-cpamt-silvia-botelho-physical-properties-diferent-soybean-cultivars-drying.pdf	
Registro original: 	Embrapa Agrossilvipastoril (CPAMT)	
Exemplares: 	CPAMT - (1286-1) - UPC - AP - DD -  -  -  - DIS