Data/hora: 06/06/2024 10:03:38

Biblioteca(s): | Embrapa Instrumentação.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | B - 1
Data corrente: | 29/12/2022
Data da última atualização: | 22/01/2024
Autoria: | Dos SANTOS, D. M.; MIGLIORINI, F. L.; SOARES, A. C.; MATTOSO, L. H. C.; OLIVEIRA, Jr., O. N.; CORREA, D. S.
Afiliação: | LUIZ HENRIQUE CAPPARELLI MATTOSO, CNPDIA; DANIEL SOUZA CORREA, CNPDIA.
Título: | Electrochemical immunosensor made with zein-based nanofibers for on-site detection of Aflatoxin B1.
Ano de publicação: | 2022
Fonte/Imprenta: | Electroanalysis, v. 34, 2022.
Páginas: | 9 p.
DOI: | doi.org/10.1002/elan.202100672
Idioma: | Inglês
Conteúdo: | A disposable electrochemical immunosensor for on-site detection of aflatoxin B1(AFB1), one of the most toxic mycotoxins in agri-food products, was fabricated through a low-cost cut-printing method and then modified with zein/polypyrrole(PPy) electrospun nanofibers onto which anti AFB1 monoclonal antibodies were immobilized covalently. Fabrication was possible with an innovative and simple approach to adsorb nanofibers onto the working electrode during electrospinning. Electrochemical impedance spectroscopy was employed as the principle of detection, and the data collected with a portable potentiostat were treated with information visualization techniques. The nanostructured immunosensor showed a high sensitivity for AFB1 with a linear detection range from 0.25 to 10 ngmL
Palavras-Chave: | Electrochemical impedance; Electrospun fibers; Food contaminants.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1150492/1/P-Electrochemical-Immunosensor-Made-with-Zein-based.pdf
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (18177-1) - UPC - AP - DD - PROCI.22/195 -  - 2022/203 - DIS