Data/hora: 12/06/2024 09:24:31

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	18/01/2006	
Data da última atualização: 	24/08/2010	
Autoria: 	ASSIS, O. B. G.; SILVA, E. R.	
Título: 	The use of electrochemical techniques for ceramic filtration medium cleaning.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	Materials Science Forum, Aedermannsdorf, v. 498-499, p. 464-469, Nov. 2005.	
Idioma: 	Inglês	
Conteúdo: 	Preliminary results of the use of eletroomosis technique for removal of organic contaminants in ceramic filtration porous structure are presented. The methods employed provokes the migration of chemical residue and waste retained or adsobed on the pore surfaces by applying a controlled tension with an electrochemical system. The results show the removal is proportional for up to 58% of the contaminant in dilluted condition.	
Palavras-Chave: 	Electrokinetic process; Electroomosis; Filter cleaning; Porous materials.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9163-1) - UPC - SP - -- - PROCI-05.00008 -  - 2005.00008 - DIS