Data/hora: 11/06/2024 23:27:06

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	20/02/2006	
Data da última atualização: 	20/02/2006	
Autoria: 	ASSIS, O. B. G.; BERTUCCI-NETO, V.; AVACA, L. A.	
Título: 	The use of electrochemcial process in soil decontamination.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON ENVIRONMENTAL FHYSICS, 1999, Brasília. [Abstracts...] Brasília: UnB-ICCMP, 1999. Não paginado.	
Idioma: 	Inglês	
Conteúdo: 	The electrochemical remediation of soils involves the application of a low direct current (on the order of mA/cm2) or low electrical potential gradient (V/cm) to a pair of positive and negative electrodes. In the presence of water, or any other specific electrolyte, the process results in migration of ions toward the electrode of opposite charge, where the contaminants under the action of the electric field are transported to the anode or the cathode and subsequently remoed for ex-situ treatment.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9417-1) - UPC - SP - -- - PROCI-99.00007 -  - 1999.00007 - DIS