Data/hora: 03/06/2024 05:14:23

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 30/03/2006
Data da última atualização: | 30/03/2006
Autoria: | ASSIS, O. B. G.; VIEIRA, D. C.; BERNARDES-FILHO, R.
Título: | AFM characterization of protein net formation on a fibrous medium.
Ano de publicação: | 2000
Fonte/Imprenta: | Brazilian Journal of Chemical Engineering, São Paulo, v.17, n.1, p.245-249, jun.2000.
Idioma: | Inglês
Conteúdo: | Lysozyme protein net is set on a glass fiber support using the self-assembly technique. Enzymatic film formation is followed by surface imaging via atomic force microscopy (AFM). Change in roughness as a function of deposition time is used as an indirect indicator of film formation. The objective was to form a protein film that would have no effect on the permeability of the medium, aiming at its application as a bioactive membrane or reactor suitable for bacteria and chemical interactions in aqueous media.
Palavras-Chave: | Protein net; Self-assembly; Thin-film.
Thesaurus Nal: | atomic force microscopy.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9702-1) - UPC - SP - -- - PROCI-00.00010 -  - 2000.00010 - DIS