Data/hora: 22/06/2024 20:52:44

Biblioteca(s): | Embrapa Gado de Leite.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | Internacional - A
Data corrente: | 23/03/2009
Data da última atualização: | 24/03/2023
Autoria: | OTENIO, M. H.; PANCHONI, L. C.; CRUZ, G. C. A.; RAVANHANI, C.; BIDÓIA, E. D.
Afiliação: | Marcelo Henrique Otênio, Embrapa Gado de Leite; Luciana Cadioli Panchoni, SAAE-PR; Gabriela Correia Araújo da Cruz, SAAE-PR; Clézio Ravanhani, SAAE-PR; Ederio Dino Bidóia, Unesp.
Título: | Avaliação em escala laboratorial da utilização do processo eletrolítico no tratamento de águas.
Ano de publicação: | 2008
Fonte/Imprenta: | Química Nova, v. 31, n. 3, p. 508-813, 2008.
Idioma: | Português
Conteúdo: | Water treatment uses chlorine for disinfection causing formation of trihalomethanes. In this work, an electrolytic water pre-treatment was studied and applied to the water from a fountainhead. The action against microorganisms was evaluated using cast-iron and aluminum electrodes. Assays were made in laboratory using the electrolytic treatment. After 5 min of electrolysis the heterotrophic bacteria count was below 500 cfu/mL and complete elimination of total and fecal coliforms was observed. Using electrolytic treatment as a pretreatment of conventional tap water treatment is proposed.
Palavras-Chave: | Tratamento eletrolítico.
Thesagro: | Desinfecção; Qualidade da Água.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/596412/1/Avaliacao-em-escala-laboratorial.pdf
Registro original: | Embrapa Gado de Leite (CNPGL)
Exemplares: | CNPGL - (16326-1) - UPC - AP - DD -  -  -  - DIS