Data/hora: 17/06/2024 08:21:13

Biblioteca(s): 	Embrapa Algodão.	
Data corrente: 	13/01/2020	
Data da última atualização: 	20/01/2020	
Autoria: 	SILVA, J. E. da; MELO, D. M. de A.; MELO, M. A. de F.; AGUIAR, E. M. de; PIMENTA, A. S.; MEDEIROS, E. P. de; CALIXTO, G. Q.; BRAGA, R. M.	
Afiliação: 	Janduir Egito da Silva, Universidade Federal do Rio Grande do Norte - UFRN; Dulce Maria de Araújo Melo, Universidade Federal do Rio Grande do Norte - UFRN/Instituto de Química; Marcus Antônio de Freitas Melo, Universidade Federal do Rio Grande do Norte - UFRN; Emerson Moreira de Aguiar, Universidade Federal do Rio Grande do Norte - UFRN; Alexandre Santos Pimenta, Universidade Federal do Rio Grande do Norte - UFRN; EVERALDO PAULO DE MEDEIROS, CNPA; Guilherme Quintela Calixto, Universidade Federal do Rio Grande do Norte - UFRN; Renata Martins Braga, Universidade Federal do Rio Grande do Norte - UFRN.	
Título: 	Energetic characterization and evaluation of briquettes produced from naturally colored cotton waste.	
Ano de publicação: 	2019	
Fonte/Imprenta: 	Environmental Science and Pollution Research, v. 26, 2019.	
Idioma: 	Inglês	
Conteúdo: 	Cotton crops generate millions of tons of lignocellulosic waste in Brazil that could be used in energy generation; however, the main destination of this raw material is soil incorporation. The aim of this work was to perform an energetic characterization and evaluation of briquettes produced from different agricultural waste of naturally colored cotton for power generation. The cultivars Brasil Sementes (BRS) Jade and Topazio were studied, with white cotton (BRS 286) as standard for comparison purposes. Two different parts of each species, stalk and cotton shell, were analyzed by bulk density, proximate analysis, higher heating value, cellulose, hemicellulose, protein, fat and lignin content, thermogravimetric analysis, and briquette mechanical strength. The results of the energetic characterization indicated a higher energetic potential of the colored species when compared with the white cotton, especially because of the volatile matter content, fixed carbon, and higher heating value. The briquette mechanical strength was higher in the samples formulated by a mixture of stalk and shell. Finally, it was concluded that the waste from colored cotton cultivars, Jade and Topazio, is capable to generate briquettes with good mechanical and physicochemical characteristics, especially those formed by the mixture of stalk and shell.	
Palavras-Chave: 	Biomass densification; Briquette mechanical strength; Energetic characterization; Natural colored cotton.	
Thesaurus Nal: 	Briquettes.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/208662/1/Energetic-Characterization-and-evaluation.pdf	
Registro original: 	Embrapa Algodão (CNPA)	
Exemplares: 	CNPA - (28695-1) - UPC - AP - DD -  -  -  - DIS