Data/hora: 23/09/2024 01:53:36

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	18/01/2005	
Data da última atualização: 	08/03/2010	
Autoria: 	CORRADINI, E.; MEDEIROS, E. S. DE; CARVALHO, A. J. F.; CURVELO, A. A. S.; MATTOSO, L. H. C.	
Título: 	Studies on dynamic mechanical properties and morphology of starch/zein blends plasticized with glycerol.	
Ano de publicação: 	2004	
Fonte/Imprenta: 	In: INTERNATIONAL SYMPOSIUM ON NATURAL POLYMERS AND COMPOSITES, 5. Anais... São Pedro: ABPol: CNPDIA/EMBRAPA: FCA/UNESP: FEQ/UNICAMP/USP, 2004. p. 346-348.	
Idioma: 	Inglês	
Conteúdo: 	Starch/zein blends were prepared varying the zein content and using glycerol as plasticizer. The blends were processed in a intensive mixer connected to a torque rheometer. The mixtures obtained were compression molder at 160°C and characterized by dinamic mechanical thermal analysis and optical microscopy. These analyses showed that the starch/zein blends are immiscible in the range of the composition studied.	
Palavras-Chave: 	DMTA; Polímeros naturais; Termoplástico.	
Thesagro: 	Zeína.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8601-1) - UPC - SP - -- - PROCI-04.00090 -  - 2004.00090 - DIS