Data/hora: 15/06/2024 00:59:14

Biblioteca(s): 	Embrapa Cerrados.	
Data corrente: 	20/09/2017	
Data da última atualização: 	02/05/2024	
Autoria: 	WOLFF, W.; DUARTE, S. N.; SOCCOL, O. J.; RODRIGUES, L. N.; FERNANDES, R. D. M.	
Afiliação: 	WAGNER WOLFF, UNIVERSIDADE DE SÃO PAULO; SERGIO NASCIMENTO DUARTE, UNIVERSIDADE DE SÃO PAULO; OLÍVIO JOSÉ SOCCOL, UNIVERSIDADE DO ESTADO DE SANTA CATARINA; LINEU NEIVA RODRIGUES, CPAC; RAFAEL DREUX MIRANDA FERNANDES, UNIVERSIDAD DE SEVILLA.	
Título: 	Methodology for rainwater reservoir dimensioning: a probabilistic approach.	
Ano de publicação: 	2017	
Fonte/Imprenta: 	Acta Scientiarum, v. 39, n. 3, p. 283-289, 2017.	
Páginas: 	p. 283-289.	
Idioma: 	Inglês	
Conteúdo: 	The aim of this study was to propose a new methodology for reservoir rainwater dimensioning based on probabilistic modeling. Eucalyptus seedlings grown in a greenhouse were used to obtain a hypothetical water demand. Meteorological data were used to estimate the demand (evapotranspiration) and offer (rainfall over the greenhouse coverage). The probability distribution of Wakeby presented the best fit for the rainfall data; therefore, a Wakeby distribution was used to model the flow-duration curve of the greenhouse coverage. For a payback period (T) of 10 years of surplus water demand and water supply deficit, a reservoir with 13.60 m³ was obtained. The proposed methodology combined the simultaneous occurrence of the events to enable the scaling out of a reservoir with high safety to supply the required demand (T = 100 years) and therefore enables a lower cost of deployment compared to each approach separately (T = 10 years).	
Thesagro: 	Irrigação.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1075920/1/Artigo-Methodology-for-rainwater-reservoir-dimensioning.pdf	
Registro original: 	Embrapa Cerrados (CPAC)	
Exemplares: 	CPAC - (35932-1) - UPC - AP - PP - S2238 -  - S2238 - DIS