Data/hora: 09/06/2024 20:54:14

Biblioteca(s): 	Embrapa Meio Ambiente.	
Data corrente: 	14/01/2008	
Data da última atualização: 	15/02/2023	
Autoria: 	ASSALIN, M. R.; FABRIN NETO, J. B.; DURÁN, N.; HAUN, M.	
Afiliação: 	Marcia Regina Assalin, Embrapa Meio Ambiente; João Batista Fabrin Neto, Departamento de Bioquímica-UNICAMP; Nelson Durán, Laboratório de Química Biológica-UNICAMP; Marcela Haun, Departamento de Bioquímica-UNICAMP.	
Título: 	Toxicity assay in kraft E1 effluent treated by ozone: algae growth inhibition and cytotoxicity in V79 cells.	
Ano de publicação: 	2007	
Fonte/Imprenta: 	Ozone: Science and Engineering, Philadelphia, v. 29, n. 1, p. 47-53, 2007.	
Idioma: 	Inglês	
Conteúdo: 	The efficiency of an ozonation process in the degradation of the Kraft E1 effluent was evaluated. The investigation was focused on the reduction of chemical oxygen demand, total phenols, color and the absorbance at 254 nm. The chronic toxicity was evaluated by growth inhibition of algae Selenatrum capricornutum and cytotoxicity evaluation of effluents samples by determination of the nucleic acid content (NCA) endpoint. After 60 minutes of ozonation, COD and UV254 only reached 21% and 34% efficiency reduction. Total phenols and color were more rapidly removed (at 10 minutes of treatment). The results showed that the chronic toxicity (Selenastrum capricornutum algae) decreases for all effluent doses studied. The cytotoxicity assay indicated that toxic compounds were not generated by the ozonation process.	
Palavras-Chave: 	Degradação; Selenatrum capricornutum.	
Thesagro: 	Alga; Ozônio; Resíduo Industrial; Toxidez; Tratamento.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Meio Ambiente (CNPMA)	
Exemplares: 	CNPMA - (7163-1) - UPC - AP - DD - Aq5 G2 - PAT 2007 - 2008.00017 - DIS