Data/hora: 23/09/2024 12:49:00

Biblioteca(s): 	Embrapa Florestas.	
Tipo da produção científica: 	Artigo em Periódico Indexado	
Circulação/Nível: 	A - 1	
Data corrente: 	25/01/2021	
Data da última atualização: 	10/03/2021	
Autoria: 	LIMA, G. G. de; FERREIRA, B. D.; MATOS, M.; PEREIRA, B. L.; NUGENT, M. J. D.; HANSEL, F. A.; MAGALHAES, W. L. E.	
Afiliação: 	GABRIEL GOETTEN DE LIMA, Programa de Pós-Graduação em Engenharia e Ciência dos Materiais, UFPR; BRUNO DIAS FERREIRA, UFPR; MAILSON MATOS, Programa de Pós-Graduação em Engenharia e Ciência dos Materiais, UFPR; BRUNO LEANDRO PEREIRA, Programa de Pós-Graduação em Engenharia e Ciência dos Materiais, UFPR; MICHAEL J. D. NUGENT, Materials Research Institute, Athlone Institute of Technology; FABRICIO AUGUSTO HANSEL, CNPF; WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF.	
Título: 	Effect of cellulose size-concentration on the structure of polyvinyl alcohol hydrogels.	
Ano de publicação: 	2020	
Fonte/Imprenta: 	Carbohydrate Polymers, v. 245, 116612, Oct. 2020. 10 p.	
DOI: 	https://doi.org/10.1016/j.carbpol.2020.116612	
Idioma: 	Inglês	
Conteúdo: 	Microfibrillated cellulose as a reinforcement agent has been investigated extensively due to their unique characteristics, which can reorder the structure of polymers and hydrogels leading to improved mechanical properties with minimal disadvantages in terms of the targeted original applications. However, effect of using a macro- to a micro-fibrillated cellulose onto polyvinyl alcohol hydrogels is still unknown, because of the unique ability for both to be produced as hydrogels from freeze-thawing mechanisms ? hydrogen bonding - there is a potential synergism. Therefore, macro and microfibrillated kraft bleached paper was synthesised at various concentrations on polyvinyl alcohol hydrogels. The overall effect presented a strong interaction between both compounds but it was increased with macrofibrillated cellulose. Increase in crystallinity was also observed with a macro-sized fibre without variation on tensile elastic modulus but an overall improvement was perceived on thermal properties and a slower swelling rate with a microfibrillated cellulose.	
Palavras-Chave: 	Celulose microfibrilada; Composite hydrogels; Compósitos hidrogéis; Congelar-descongelar; Freeze-thawing; Kraft process; Microfibrillated cellulose; PVA.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (57562-1) - UPC - AP - DD -  -  -  - DIS