Data/hora: 24/06/2024 17:58:43

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 20/01/2005
Data da última atualização: | 08/03/2010
Autoria: | MARTINS, M. A.; JOEKES, I.; FERREIRA, F. C.; JOB, A. E.; MATTOSO, L. H. C.
Título: | Thermal behavior of raw and chemically treated sisal fibers.
Ano de publicação: | 2004
Fonte/Imprenta: | In: INTERNATIONAL SYMPOSIUM ON NATURAL POLYMERS AND COMPOSITES, 5. Anais... São Pedro: ABPol: CNPDIA/EMBRAPA: FCA/UNESP: FEQ/UNICAMP/USP, 2004. p. 13-15.
Idioma: | Inglês
Conteúdo: | Abstract: In this work  mercerization, acetylation, and resorcinol/hexamethylenetetra- mine (R/H) solution treatments have been applied to sisal fibers to enhance adhesion with polymer matrices in composite materiais. The thermal behavior of raw and chemi- cally treated sisal fibers has been studied using the thermal gravimetric analysis (TGA) and the differential thermal gravimetry (DTG). The value of the initial decomposition temperature of sisal has been found to increase as a result of mercerization/acetylation treatment. Moreover, the rate ofthermal degradation offibers treated with RIH solution has beenfound to be lower than those of the raw fibers.
Palavras-Chave: | Fibra de sisal; TGA; Tratamento químico.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (8603-1) - UMT - SP - -- - PROCI-04.00091 -  - 2004.00091 - DIS